** RP-ALARA Association**

PLANT STATUS REPORT QUESTIONAIRE – Year\_2022\_

STATION: \_Callaway\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

UTILITY: \_\_Ameren Missouri\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Prepared By: \_\_Aaron Enloe/Adam Gilliam\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **CYCLE**  **#** | **Previous Year**  **ON-LINE DOSE**  **(Rem-DLR)** | **RWP**  **person hours** | **ONLINE Level 2&3 PCE'S** |
| **UNIT 1** | 25 | 3.32 | 92,313 | 1 |
| **UNIT 2** |  |  |  |  |
| **UNIT 3** |  |  |  |  |
| **RW/Common** |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | **LAST REFUEL OUTAGE EXPOSURE**  **ESTIMATE / ACTUAL (Rem-DLR)** | **DURATION**  **ESTIMATE / ACTUAL** | **Level**  **2&3**  **PCE's** |
| **UNIT 1** | 26.7/22.477 | 55/79.3 | 0 |
| **UNIT 2** |  |  |  |
| **UNIT 3** |  |  |  |
| **UNIT 4** |  |  |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SPECIALTY RESIN** |  |  | **TYPE OF RESIN:** | **USED DURING: S/D CLEANUP** |  | **ONLINE** |  |  |
| **RCS FILTRATION MICRON SIZE: ON-LINE: .1 DURING SHUTDOWN CLEANUP:**  **1** | | | | | | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Previous Year** | **LOWEST and HIGHEST CANISTER DOSE (Rem)** | **HIGHEST KW & BURNUP CASK** | **NUMBER OF CANISTERS** | **VENDOR** | **CANISTER TYPE** |
| **DRY FUEL**  **STORAGE CAMPAIGN** | 0.225 Rem / 0.450 Rem |  | 12 | Holtec | HiStorm |

**Additional Comments:**